
***WOODWIND CARE***

***Flute / Piccolo Care***

**Daily Care**


1. When removing your flute from its case never pick it up by its keys. Remove it by the ends where there are no keys.

2. Put the flute together with a slow back-and-forth twisting motion, never push or pull the flute when assembling or disassembling this can cause the instrument to become bent at the joints.



3. Each time you put the flute together a small amount of debris will build-up on the tenons (this is normal), however, this can make it difficult to assemble. Always wipe the tenons (joints) with a soft cloth before assembling. (Fig.1)

4. The use of lubricants on the tenons is not recommended - this can cause damage over time. (The only exception to this rule is on some piccolos and wood flutes that have cork joints. You should apply a small amount of cork grease to these joints, as needed, to aid in assembly).



5. After you are finished playing, use a cleaning rod with an absorbent cloth to swab out the inside of all parts to remove moisture. (Fig.2) Carefully wipe off the outside of the flute to remove oils or perspiration caused by your hands.

6. Always store your flute in its case when not in use, this helps prevent damage and aids in keeping the instrument from tarnishing. Do not place anything in the case that can press on the flute, this can bend keys.

**Monthly Care**

Check all screws and pivots to see if they are coming loose. If they are, take your flute to your tutor to have them adjusted. It is not suggested that you try and adjust them yourself because they can be over tightened or damaged.

<http://www.musiccenters.com/care.html>